|  |  |
| --- | --- |
| Izpolni naročnik – organizator prevoza / To be filled out by client | **KONTROLNI LIST PRED NAKLADANJEM NEVARNEGA BLAGA – V VOZILU CISTERNI**  CHECK FORM BEFORE LOADING DANGEROUS GOODS – IN TANK VEHICLE  V KOLIKOR JE NA PREVOZNI ENOTI ŽE NALOŽENO NEVARNO BLAGO – UPOŠTEVATI ZAHTEVE O DOPUSTNEM POLNJENJU V SOSEDNJA PREKATA  IN CASE THE TRANSPORT UNIT IS ALREADY LOADED WITH DANGEROUS GOODS – COMPLY TO REQUIREMENTS ON ALLOWABLE FILLING IN ADJOINING COMPARTMENTS A. SPLOŠNI PODATKI 1. Registrska št. vozila / priklopnika \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Registration no. Vehicle / trailer    2. Tip vozila / mesto polnjenja (obkroži ustrezno)  Type of vehicle / filling point (circle the appropriate)  3. Voznik (ime in priimek) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Driver (name and surname)  4. UN številka/razred /embalažna skupina \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  UN number/class/packing group (navedite podatke ali priložite fotokopijo CMR listine /  provide information or attach a photocopy of the CMR list)  5. Količina naloženega nevarnega blaga PO SPREMLJAJOČI DOKUMENTACIJI  Amount of loaded dangerous goods ACCORDING TO ACCOMPANYING DOCUMENTATION  6. Zadnji prevažan tovor \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Last transported cargo  7. Cisterna je bila oprana (datum, kraj) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  The tank was washed (date, place) B. KONTROLA DOKUMENTOV IN VOZILA 1. Veljavnost ADR: Vozilo\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, Priklopnik\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Validity of ADR: Vehicle Trailer  2. Certifikat ADR o usposobljenosti voznika \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Drivers certificate of ADR competence  3. Delujoče sonde proti prepolnitvi DA NE  Working overfill probes  4. Listina o prevozu nevarnega blaga DA NE  Document on the transport of dangerous goods  NAROČNIK  CUSTOMER/CLIENT  Kraj in datum \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_ /\_\_\_ / 20\_\_\_  Place and date |
| Izpolni voznik / driver | C. POTRJUJEM:Da vozilo ustreza zahtevam za prevoz nevarnega blaga (oprema vozila, oranžne table in nalepke nevarnosti), da je cisterna ustrezna za to vrsto nevarne snovi in nima ostankov druge snovi ter da je na vsakem prekatu cisterne delujoča sonda proti prepolnitvi. V kabini vozila so pisna navodila po ADR. I CERTIFY: That the vehicle complies with the requirements for the transport of dangerous goods (equipment, orange-coloured plates and placards), that the tank is appropriate for the type of dangerous goods, has no residue of other substances, and that there is a working overfill probe on each compartment of the tank. Instructions in writing according to ADR are in the cabin of the vehicle. VOZNIK / DRIVER |